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TONGLI MINING TRUCK PARTS
Leaf Spring Slider Seat
Part No. 87029110091  ·  Cast-Steel Reinforced  ·  OEM-Spec Replacement
	Part Number
	87029110091

	Product
	Leaf Spring Slider Seat (Cast-Steel Spring Base Plate)

	Material
	High-Strength Cast Steel, Anti-Corrosion Coated

	Brand
	Tongli (TONLY) Mining Truck

	Fitment
	TL875B · TLE105 · TLE135 · 875D · 883 · 885

	Position
	Rear Leaf Spring Slider / Spring Seat

	MOQ
	1 PC — Sample & Wholesale Welcome

	Lead Time
	In Stock — Ships Within 48 Hours



1. Product Overview
The Leaf Spring Slider Seat (P/N 87029110091) is a mission-critical chassis component engineered for Tongli (TONLY) wide-body mining dump trucks. Machined from high-strength cast steel and finished with anti-corrosion coating, it serves as the load-bearing interface between the leaf spring pack and the axle housing — absorbing continuous shock, torsion and vibration under the most punishing off-road mining conditions.
Designed to OEM specifications, this slider seat guarantees a 100% bolt-on fit with zero on-site machining. Whether you operate a single TL875B or manage an entire fleet of TLE-series electric mining trucks, part 87029110091 delivers the durability, alignment precision and service life your operation demands.

2. Key Selling Points
1. ✅ OEM-Exact Fit — Engineered to original Tongli blueprint 87029110091. Direct replacement for TL875B, TLE105, TLE135 and 875D/883/885. No modification, no guesswork.
1. ✅ Cast-Steel Reinforced Body — Forged from high-strength cast steel to withstand heavy shock loads, extreme torsion and constant vibration in open-pit mining.
1. ✅ Precision Bolt Pattern — Pre-drilled holes match original bolting layout exactly — perfect alignment, bolt-on in under 30 minutes.
1. ✅ Anti-Corrosion Protection — Multi-stage surface treatment (shot-blast + primer + powder coat) resists rust, road salt, slurry and humidity.
1. ✅ Wear-Resistant Slider Face — Hardened and finely machined contact surface reduces friction against the leaf spring, extending spring life.
1. ✅ Rig-Tested Durability — Each batch load-tested to simulate 10,000+ hours of mining-duty cycles — zero cracking or fatigue failure.
1. ✅ Ready Stock & Fast Dispatch — Warehoused for immediate shipment. Small MOQ supported for overseas workshops and fleet operators.
1. ✅ Neutral or Branded Packing — Available in neutral export carton or Tongli-label packing to suit aftermarket or OEM resale.

3. Technical Specifications
	Specification
	Detail

	Part Number
	87029110091

	Description
	Leaf Spring Slider Seat / Cast-Steel Spring Base Plate

	Material
	High-Strength Cast Steel (ZG270-500 equivalent)

	Surface Treatment
	Shot Blasting + Anti-Rust Primer + Powder Coating

	Slider Face Hardness
	HRC 45–55 (wear-resistant)

	Mounting
	Pre-drilled holes, M20 Grade 8.8 bolts recommended

	Fitment
	TL875B · TLE105 · TLE135 · 875D · 883 · 885

	Application
	Rear suspension leaf spring slider / spring seat

	Operating Environment
	Open-pit mines, quarries, heavy haul roads

	Typical Service Life
	6,000 – 10,000 hours under standard mining cycles

	Warranty
	12 months / 6,000 hours (whichever first)

	Packaging
	Neutral carton / Wooden crate (bulk orders)

	Gross Weight
	Approx. 18 – 22 kg / piece



4. Vehicle Fitment
	Model
	Engine / Powertrain
	Payload
	Fuel Type

	TL875B
	Weichai 430 HP
	60 Tons
	Diesel

	TLE105
	CAT / Weichai Electric
	70 Tons
	Battery Electric

	TLE135
	CAT / Weichai Electric
	90 Tons
	Battery Electric (Autonomous)

	875D / 883 / 885
	Weichai / Cummins
	60–80 Tons
	Diesel



⚠  Always confirm fitment by sending your VIN plate photo or old part number. Technical team responds within 2 hours.

5. Why Choose Us
1. ⭐ 20+ Years of Expertise — Specialized in Chinese heavy-duty & mining truck spare parts since 2003.
1. ⭐ 100% Genuine & OEM-Spec — Every part sourced from certified manufacturers or genuine OEM channels.
1. ⭐ Rigorous QC — Dimensional check, hardness test, coating thickness test on every batch.
1. ⭐ Global Shipping — DHL / FedEx for urgent samples; sea freight for bulk container orders.
1. ⭐ Multilingual Support — English, Russian, Spanish, Arabic, French, German, Portuguese.
1. ⭐ After-Sales Warranty — 12-month warranty with replacement guarantee for manufacturing defects.

6. Ordering Information
	Item
	Detail

	Part Number
	87029110091

	MOQ
	1 Piece (Sample accepted)

	Wholesale Pricing
	Tiered discount for 10+ / 50+ / 100+ pcs — request quote

	Payment Terms
	T/T · Western Union · PayPal · L/C (bulk)

	Delivery Time
	In stock → dispatched within 48 hours

	Shipping Methods
	DHL / FedEx / UPS (air) · Sea freight (bulk)

	Export Ports
	Qingdao / Shanghai / Tianjin, China

	Packaging Options
	Neutral carton / Tongli branded / Wooden crate



7. Get a Quote
Ready to order or need fitment confirmation? Contact us today:
1. 📧 Send VIN plate photo or old part number → fitment confirmed within 2 hours
1. 📦 Request a sample or wholesale quote for P/N 87029110091
1. 🌍 Worldwide shipping via DHL / FedEx / sea freight — door-to-door available
1. 💬 WhatsApp / WeChat / Email support in 7 languages

	📩  CONTACT US NOW FOR A COMPETITIVE QUOTE
Part No. 87029110091  ·  Tongli Mining Truck Leaf Spring Slider Seat



SEO Keywords
87029110091, Tongli leaf spring slider seat, TONGLI TL875B parts, mining truck spring seat, cast steel spring base plate, wide body mining truck spare parts, TONLY 87029110091, leaf spring slider seat China supplier, mining dump truck undercarriage parts
© Tongli Mining Truck Spare Parts Supplier  |  All specs subject to change without notice  |  Verify fitment before purchase
